## Name

host — DNS lookup utility

## Synopsis

`host` [`-aCdlnrsTwv`] [`-c `class``] [`-N `ndots``] [`-R `number``] [`-t `type``] [`-W `wait``] [`-m `flag``] [`-4`] [`-6`] {name} [server]

## DESCRIPTION

host is a simple utility for performing DNS lookups. It is normally used to convert names to IP addresses and vice versa. When no arguments or options are given, host prints a short summary of its command line arguments and options.

`name` is the domain name that is to be looked up. It can also be a dotted-decimal IPv4 address or a colon-delimited IPv6 address, in which case host will by default perform a reverse lookup for that address. `server` is an optional argument which is either the name or IP address of the name server that host should query instead of the server or servers listed in `/etc/resolv.conf`.

The `-a` (all) option is equivalent to setting the `-v` option and asking host to make a query of type ANY.

When the `-C` option is used, host will attempt to display the SOA records for zone `name` from all the listed authoritative name servers for that zone. The list of name servers is defined by the NS records that are found for the zone.

The `-c` option instructs to make a DNS query of class `class`. This can be used to lookup Hesiod or Chaosnet class resource records. The default class is IN (Internet).

Verbose output is generated by host when the `-d` or `-v` option is used. The two options are equivalent. They have been provided for backwards compatibility. In previous versions, the `-d` option switched on debugging traces and `-v` enabled verbose output.

List mode is selected by the `-l` option. This makes host perform a zone transfer for zone `name`. Transfer the zone printing out the NS, PTR and address records (A/AAAA). If combined with `-a` all records will be printed.

The `-i` option specifies that reverse lookups of IPv6 addresses should use the IP6.INT domain as defined in RFC1886. The default is to use IP6.ARPA.

The `-N` option sets the number of dots that have to be in `name` for it to be considered absolute. The default value is that defined using the ndots statement in `/etc/resolv.conf`, or 1 if no ndots statement is present. Names with fewer dots are interpreted as relative names and will be searched for in the domains listed in the search or domain directive in `/etc/resolv.conf`.

The number of UDP retries for a lookup can be changed with the `-R` option. `number` indicates how many times host will repeat a query that does not get answered. The default number of retries is 1. If `number` is negative or zero, the number of retries will default to 1.

Non-recursive queries can be made via the `-r` option. Setting this option clears the RD — recursion desired — bit in the query which host makes. This should mean that the name server receiving the query will not attempt to resolve `name`. The `-r` option enables host to mimic the behavior of a name server by making non-recursive queries and expecting to receive answers to those queries that are usually referrals to other name servers.

By default, host uses UDP when making queries. The `-T` option makes it use a TCP connection when querying the name server. TCP will be automatically selected for queries that require it, such as zone transfer (AXFR) requests.

The `-4` option forces host to only use IPv4 query transport. The `-6` option forces host to only use IPv6 query transport.

The `-t` option is used to select the query type. `type` can be any recognized query type: CNAME, NS, SOA, SIG, KEY, AXFR, etc. When no query type is specified, host automatically selects an appropriate query type. By default, it looks for A, AAAA, and MX records, but if the `-C` option was given, queries will be made for SOA records, and if `name` is a dotted-decimal IPv4 address or colon-delimited IPv6 address, host will query for PTR records. If a query type of IXFR is chosen the starting serial number can be specified by appending an equal followed by the starting serial number (e.g. -t IXFR=12345678).

The time to wait for a reply can be controlled through the `-W` and `-w` options. The `-W` option makes host wait for `wait` seconds. If `wait` is less than one, the wait interval is set to one second. When the `-w` option is used, host will effectively wait forever for a reply. The time to wait for a response will be set to the number of seconds given by the hardware's maximum value for an integer quantity.

The `-s` option tells host not to send the query to the next nameserver if any server responds with a SERVFAIL response, which is the reverse of normal stub resolver behavior.

The `-m` can be used to set the memory usage debugging flags `record`, `usage` and `trace`.

## IDN SUPPORT

If host has been built with IDN (internationalized domain name) support, it can accept and display non-ASCII domain names. host appropriately converts character encoding of domain name before sending a request to DNS server or displaying a reply from the server. If you'd like to turn off the IDN support for some reason, defines the `IDN_DISABLE` environment variable. The IDN support is disabled if the variable is set when host runs.

## FILES

`/etc/resolv.conf`

## SEE ALSO

dig(1), named(8).